{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":11,"n_cols":6,"rows_kept":11,"merged":[[0,0,0,5]],"flags":["formulas_cached_only"]}
["昆明技师学院本部二级供水泵维修维护内容及技术参数"]
["序号","名称","规格型号","数量","单位","备注"]
[1,"不锈钢立式多级离心泵","IGF45-62-11；流量45m³/h；扬程62m；功率11kW；转速2900r/min。",2,"台","更换多级离心泵（含电动机）；提供检测报告。"]
[2,"变频控制柜","变频控制器，一控二，PLC",1,"套","提供检测报告。"]
[3,"稳压罐","不锈钢材质，容积≧1立方，正国标",1,"个","提供检测报告"]
[4,"阀门","正国标",4,"个","与管径适配；提供检测报告"]
[5,"止回阀","正国标",2,"个","与管径适配；提供检测报告"]
[6,"金属连接件","正国标",4,"个","与管径适配；提供检测报告"]
[7,"压力传感器","正国标",1,"个","提供检测报告"]
[8,"更换供水管道","镀锌管DN100,正国标",10,"米","提供检测报告"]
[9,"维修原离心泵",null,2,"台","对原离心泵（含电动机）进行维修维护，修复后备用。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}