{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":40,"n_cols":8,"rows_kept":40,"merged":[[0,0,0,7]],"flags":["formulas_cached_only"]}
["昆明技师学院西校区食堂设备维修维护服务清单"]
["序号","设备名称","单位","数量","设备尺寸","安放位置","主要维修维护内容","备注"]
[1,"四人位餐桌","套",35,null,"餐厅","焊接打磨凳支撑架，更换脚套"]
[2,"双门玻璃门消毒柜","台",1,"1380*625*1800","餐厅","需维修密封条，灯管、风机"]
[3,"双层平板工作台","台",1,"1800*700*800","备餐间","更换调节脚，焊接支撑梁"]
[4,"双层平板工作台","台",1,"1250*700*800","备餐间","更换调节脚，焊接支撑梁"]
[5,"五格售饭台","台",2,"1800*700*800","售卖间","更换调节脚，更换发热管、更换温控、更换指示灯"]
[6,"单通工作台","台",1,"1800*800*800","售卖间","更换调节重力脚，调节焊接打磨门"]
[7,"冷藏操作台","台",1,"1800*760*800","售卖间","更换密封条、更换层架、更换指示灯"]
[8,"不锈钢汤桶","台",2,"1400*730*1200","售卖间","更换发热管"]
[9,"单孔蒸汽炉","台",1,"650*650*740","售卖间","更换温控"]
[10,"平板铁架","台",1,"1200*500*1800","副食仓库","焊接支撑脚，加固支撑梁"]
[11,"平板铁架","台",2,"1500*500*1800","副食仓库","焊接支撑脚，加固支撑梁"]
[12,"四层栅格层架","台",1,"1500*500*1500","烹饪间","更换调节脚"]
[13,"双层平板工作台","台",1,"1800*700*800","烹饪间","更换调节脚，焊接支撑梁"]
[14,"炉拼台","台",2,"400*1150*800+400","烹饪间","更换调节脚，切割原有焊接"]
[15,"电磁双头大锅灶","台",1,"2000*1150*800+400","烹饪间","更换显示板、更换调节手柄"]
[16,"电磁单头大锅炉","台",1,"1000*1150*800+400","烹饪间","更换调节手柄"]
[17,"电磁双头平头炉","台",1,"1400*850*530+670","烹饪间","更换显示板、更换调节手柄"]
[18,"四层栅格层架","台",1,"1200*500*1500","烹饪间","更换调节脚"]
[19,"双星工作台","台",2,"1500*700*800+150","粗加工间","更换调节脚，更换下水器、下水管"]
[20,"小型多用切菜机","台",1,"500*500*610","粗加工间","更换刀片"]
[21,"土豆脱皮机","台",1,"730*530*970","粗加工间","更换轴承"]
[22,"四层栅格层架","台",1,"1500*500*1500","粗加工间","更换调节脚"]
[23,"四门碗柜","台",1,"1200*500*1800","粗加工间","更换调节重力脚，调节焊接打磨门"]
[24,"电力24盘蒸饭车","台",1,"1390*620*1540","蒸饭间","更换指示灯，更换发热管，更换浮球阀，更换活动轮"]
[25,"电力12盘蒸饭车","台",1,"710*620*1540","蒸饭间","更换指示灯，更换发热管，更换浮球阀，更换活动轮"]
[26,"米面架","台",1,"1800*1200*250","蒸饭间","切割长度，重新焊接框架，更换调节脚。"]
[27,"拆卸、运输、安装、调试","项",1,null,null,"富民县东元食品工业园区至西山区下普坪174号","以上26项"]
[28,"灭蝇灯","台",9,"白色，36CM长","食堂内内","对原有设备进行维修改造","正国标"]
[29,"挡鼠板","台",2,"1500*25*630，不锈钢材质，厚度≧1.0㎜","食堂内","对原有设备进行维修改造","正国标"]
[30,"四格保温售饭台","台",1,"1650*700*800","售卖间","对原有设备进行维修改造","正国标"]
[31,"四格保温售饭台","台",1,"1600*700*800","售卖间","对原有设备进行维修改造","正国标"]
[32,"风幕机","台",1,"1500*182*221","售卖间","对原有设备进行维修改造","正国标"]
[33,"风幕机","台",1,"900*120.1*200","粗加工间","对原有设备进行维修改造","正国标"]
[34,"单门留样柜","台",1,"620*595*1845 ","售卖间","对原有设备进行维修改造","正国标"]
[35,"四层平板货架","架",3,"1200*500*1500","调味品仓库","对原有设备进行维修改造","正国标"]
[36,"单层地架","架",2,"1500*600*150","调味品仓库","对原有设备进行维修改造","正国标"]
[37,"工具存放架","台",1,"1500*87*200，不锈钢材质，厚度≧1.0㎜","烹饪间","对原有设备进行维修改造","正国标"]
[38,"大单星水池","台",1,"1000*700*800+150","粗加工间","对原有设备进行维修改造","正国标"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}